# The two lower address registers
vme_addr_arr += ( "0x0070000c",
                  "0x0070000e" )

