# The two lower address registers
vme_addr_arr += ( "0x0078000c",
                  "0x0078000e" )

