%
%        1         2         3         4         5         6         7         8
%2345678901234567890123456789012345678901234567890123456789012345678901234567890
%
\documentstyle[12pt]{article}
\topmargin -0.7in
\textheight 9.0in
\textwidth 6.5in
\oddsidemargin 0.0in
\evensidemargin 0.0in
\parindent 0.0in
\def\baselinestretch{1.0}
%
\begin{document}
\pagestyle{plain}
\begin{verbatim}


Hub Module    Front Panel

Rev.  14-Dec-2017


Please mill the indicated holes and rectangular cutouts
in the blank front panel for the Hub Module.

This work is for Wade Fisher and is on account:  RC104022


Changes since the Hub Module Front Panels that you
made earlier this year:

 - The front panels that you made in the spring of 2017
   had 6 holes for 4-40 screws.  The 2 holes near the
   center of the panel have been changed from 4-40 to a
   2-56 body drill  and  have been moved slightly in
   the X dimension.

   The new design has 4 holes for 4-40 screws and
   2 holes for 2-56 screws.


 - The new design has 6 holes or notches in the
   wide side wall of the panel.  The design from last
   spring had no holes or notches in this side wall.


Quantity:  28 finished front panels


The locations of the Holes and Cutouts are indicated in
the attached 8 drawings and in the following tables.



Small LED Holes:
----------------

   48 Holes

   Estimate of required diameter:  2.10 mm,  82 mills,  #45

   Please see the example  8x Light Pipe

   X,Y Hole Locations in mm:

          -10.260,  215.815
           -7.720,  215.815
           -5.180,  215.815
           -2.640,  215.815

          -10.260,  220.895
           -7.720,  220.895
           -5.180,  220.895
           -2.640,  220.895

          -10.260,  247.055
           -7.720,  247.055
           -5.180,  247.055
           -2.640,  247.055

          -10.260,  252.135
           -7.720,  252.135
           -5.180,  252.135
           -2.640,  252.135

          -10.260,  257.215
           -7.720,  257.215
           -5.180,  257.215
           -2.640,  257.215

          -10.260,  262.295
           -7.720,  262.295
           -5.180,  262.295
           -2.640,  262.295

          -10.260,  267.375
           -7.720,  267.375
           -5.180,  267.375
           -2.640,  267.375

          -10.260,  272.455
           -7.720,  272.455
           -5.180,  272.455
           -2.640,  272.455

          -10.260,  277.535
           -7.720,  277.535
           -5.180,  277.535
           -2.640,  277.535

          -10.260,  282.615
           -7.720,  282.615
           -5.180,  282.615
           -2.640,  282.615

          -10.260,  287.695
           -7.720,  287.695
           -5.180,  287.695
           -2.640,  287.695

          -10.260,  292.775
           -7.720,  292.775
           -5.180,  292.775
           -2.640,  292.775





Large LED Holes:
----------------

   6 Holes

   Estimate of required diameter:  3.25 mm,  128 mills,  #30

   Please see the example  single Light Pipe

   X,Y Hole Locations in mm:

           -7.720,   57.625
           -7.720,  202.775
           -7.720,  207.855
           -7.720,  228.895
           -7.720,  233.975
           -7.720,  239.055





4-40 Machine Screw Body Drills:
-------------------------------

   4 Holes   <---- This is a CHANGE.   Was 6 holes.

   Diameter:  4-40 body drill

   X,Y Hole Locations in mm:

           -5.800,    7.275
           -5.800,   15.075

           -8.800,  300.575
            3.200,  300.575



2-56 Machine Screw Body Drills:
-------------------------------

   2 Holes   <---- This is a CHANGE.   2 new holes.

   Diameter:  2-56 body drill

   X,Y Hole Locations in mm:

           -9.100,  159.800
           -9.100,  168.800



Rectangular Cutouts:
--------------------

   RJ1 Cutout:

           -4.600,  116.775     Center

            7.340,  125.225     Upper-Right corner
          -16.540,  125.225     Upper-Left  corner
          -16.540,  108.325     Lower-Left  corner
            7.340,  108.325     Lower-Right corner


   RJ2 Cutout:

           -4.600,   94.775     Center

            7.340,  103.225     Upper-Right corner
          -16.540,  103.225     Upper-Left  corner
          -16.540,   86.325     Lower-Left  corner
            7.340,   86.325     Lower-Right corner


   RJ3 Cutout:

           -4.600,   72.775     Center

            7.340,   81.225     Upper-Right corner
          -16.540,   81.225     Upper-Left  corner
          -16.540,   64.325     Lower-Left  corner
            7.340,   64.325     Lower-Right corner



    J2 Cutout:

           -9.450,   40.775     Center

           -6.200,   50.275     Upper-Right corner
          -12.700,   50.275     Upper-Left  corner
          -12.700,   31.275     Lower-Left  corner
           -6.200,   31.275     Lower-Right corner



LEMO Double D Hole:
-------------------

   1 Hole   Fancy double D shape

   Diameter:  please see drawing M7

   X,Y Hole Location in mm:

            2.700,   40.775


\end{verbatim}

\end{document}


