DAC LOADING

Clock

Card Level Addressing

0110 1010 0110 0000 0110 STATE MACHINE

DAC LOADING Control Signals

11 00 11 PAL -> FPGA Signals 11 00 11 11 00 11

0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 sysreset_debounced_int_stdl

pal_bx_clock_in_stdl

valid_cycle_int_stdl

OCB_ADRS(1:4) 0110 1010 0110 0000 0110

ltchd_write_b_in_stdl next_state_quiescent_int_stdl idle_state_int_stdl latch_1_state_int_stdl latch_2_state_int_stdl

io_1_state_int_stdl io_2_state_int_stdl set_quiescent_state_int_stdl

enable_fpga_configuration_reg_stdl configure_fpgas_int_stdl cnfg_prog_b_req_reg_stdlv 11 00 11

cnfg_prog_b_out_stdlv 11 00 11 cnfg_cs_b_reg_stdlv 11 00 11 cnfg_rdwr_b_reg_stdl

cnfg_cclk_out_stdl

Entity:bcp Architecture:bcp_structural Date: Mon Sep 20 11:07:39 Eastern Daylight Time 2004 Row: 1 Page: 1