State Machine Clock

INPUTS

STATE MACHINE

OUTPUTS

0 5 10 15 20 25 30 pal_bx_clock_in_stdl

valid_cycle_int_stdl ds1_int_stdl sysreset_debounced_int_stdl

idle_state_int_stdl latch_1_state_int_stdl latch_2_state_int_stdl io_1_state_int_stdl io_2_state_int_stdl set_quiescent_state_int_stdl

next_state_quiescent_int_stdl

vme_ltch_clk_out_stdl drv_dtack_out_stdl

Entity:bcp Architecture:bcp_structural Date: Sun Sep 19 18:26:55 Eastern Daylight Time 2004 Row: 1 Page: 1