U S

J a) Entry bundles

b) Exit Modes

c) Mid-route maneuvers loops

PMT location

L =

116

85

85

MODE 1 MODE 2

Ruler

R = 60

R = 45

2 L

2 L

L

Fig. 3 Fiber routing elements: a) the entry path showing the typical sub-bundle of fibers, b)˚the exit paths from neighboring loops or from the loop below the exit location, c)˚the mid-route possibilities; straight ahead (J), a u-turn (U), or a lane switch (S)