ATLAS IC ScintillatorR. MillerDimensions are in mm with a tolerance of – 0.1 unless stated otherwise. Dimensions in parentheses are in InchesDRAWNDATEPROJECTMATERIALTITLEDWG. NOSCALE

NOTES:1.

MICHIGAN STATE UNIVERSITY HIGH ENERGY PHYSICS REV 1/32" Alum SheetCOVERS

B (inside)34 – 1/16 A (inside)

1/4 – 1/32 (outside)

6-22-00c1/4 – 1/32 (outside) Dimensions – 1/32

ABBottom Cover: 8 11/16 5 11/32Top Cover: 8 25/32 5 7/161:5HEP-B-025-372

1. Top Cover should fit over Bottom Cover with edges A and B aligned2. Inside radius of bends must be less than 1/163. Edges must be straight to – 1/324. Surface must be flat to – 1/16