ATLAS IC Scintillator

R. Miller

Dimensions are in mm with a tolerance of – 0.1 unless stated otherwise. Dimensions in parentheses are in Inches

NOTES: 1.

MICHIGAN STATE UNIVERSITY HIGH ENERGY PHYSICS REV DRAWN DATE PROJECT MATERIAL TITLE DWG. NO SCALE

DXmax = 227.5

DR = 884.5

DXmin = 140.5

TileCal EB

Z=3500

Z=3480

R=1452

InterCryostat Scintillator

InterTilecal Scintilator

LAr Cryostat

INTER-CRYOSTAT SCINTILLATOR MOUNTING

143.5

117.5

R-PHI VIEW R-Z VIEW

Pin aligns inner end to slot in next ctr.

6-26-98 A

MOUNTING

HEP-B-025-371 1:5

2. Dimensions assume 2 mm between Ctrs.

R=2280

R=2250

8

15

(1)

(1/2)

20

R=2305

MOUNTING DETAIL

(2) (1/4)

(2) (#8-32 X 3/4) Socket Hd. CS attaches ICS ctr. to bracket

(2) (1/4-20 x 3/4) Socket Hd. CS Ctrbore mounts ITC ctr to EB end plate

(2 )(1/4-20 x 3/4) Flat Hd. MS Ctrsunk attaches bracket to ITC ctr.

Integral to ITC ctr.

Shim as needed to clear Cryost.

eta=1.20

Bracket

Integral to ICS ctr.

R=2280

R=2250