10 clear fibers welded to fibers from higher eta section

10 clear fibers welded to WLS fibers from lower eta section

All edges except those with fibers are mirrored, (both eta sections)

20 fiber connector

Space for source tubes fiber guide layer, 2 mm thick plastic

14 mm

10 mm thick Scintillator,

Conceptual Design of Scintillator for the Gap Region

End Piece attaches to EB end plate

End Piece attaches to

EB end plate

Covering eta sections 1.0-1.1 and 1.1-1.2

2 pieces per h

Aluminum cover,

.0.75 mm thick

Fibers exit through a light seal in the end piece. They have enough freedom of motion to allow the connection to the EB plug calorimeter

5 WLS fibers along each of these scintillator edges

Section View (x 2)