Welded seam

Masking

(printed on interior surface)

Both ends open

SLEEVE #

1224

214

99.02233

224

99.03243

233

99.04257

245

129.0

5270

257

6283

270

7296

282

149.0

8312

298

9325

310

10343

324

189.0

11362

343

A – 1 (mm)B – 1 (mm)H +0.5 -0.0 (mm)=AHB15 – 1 mm=(2 holes)11 mm dia.thru bothlayers15 – 1 mm=MICHIGAN STATE UNIVERSITY

HIGH ENERGY PHYSICS

REV.

SCALE

DWG. NO.

TITLE

PARTS LIST

PART NO.

ITEM

DESCRIPTION

QTY.ORIG

.DRAWN

PROJECT

MATERIAL

UNLESS SPECIFIED:

DECIMALS

–FRACTNS –

ANGLES –

DO NOT

SCALE DWG

R. Miller

ATLAS TileCal

Tyvek 1055B

Tile Sleeves

HEP01-024-352

8-16-97– 1 mm