ATLAS IC ScintillatorR. MillerDimensions are in mm with a tolerance of – 0.1 unless stated otherwise. Dimensions in parentheses are in InchesDRAWNDATEPROJECTMATERIALTITLEDWG. NOSCALE

NOTES:1.

MICHIGAN STATE UNIVERSITY HIGH ENERGY PHYSICS REV ASSEMBLY

(6) WLS Fibersfor cell A

BAHEP-B-025-368

227140885Mounting bracketOuter End pieceOptical connectorsockets (2) pinned and sealed into end piece

Bottom cover panel is epoxied to end pieces.Black felt light seals line the surfaces in contact with fibers or scintillator edges.Top cover panel overlaps the bottom cover and end pieces and is taped at the edges.

Compression plate with set screws in same holes as mounting screws

6 mm thickPVT Scintillator, wrapped in Tyvek

OpticalIsolators or reflectors on edges as necessary

(6) WLS Fibersfor cell B

Inner End piece

Cell B478Cell A36213

6-20-001:5B

(1/8 x 3/4) pinA